Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_EnablePreferMasterTimeEncoderEnabled | ( | GoSetup | setup,
|  | kBool | enable
| ) |  |

Sets whether the time and encoder values are preferred to come from the Master rather than from the sensor and its I/O port.

Version
  Introduced in firmware 4.8.2.76

Parameters

  setup | GoSetup object.
  enable | kBool kTrue to enable kFalse to disable.

Returns
  kStatus if enabling has been successful